In the specified concentrations, ferrosilicon is only subject to the provisions of Class 4.3 of ADN when transported in bulk or without packaging by inland
navigation vessels. If the substance is transported in bulk in vehicles, railway wagons or containers on inland waterways, it is not subject to the requirements of ADN.