According to 2.2.2.2.2 sixth indent, Aerosols where gases which are toxic according to 2.2.2.1.5 or pyrophoric according to packing instruction P200 in 4.1.4.1 are used as propellants, shall not be accepted for carriage.

According to 6.2.6.1.2 of the ADR in conjunction with section 6.1.1 of the ADN, the capacity of receptacles made of metal shall not exceed 1 000 ml; that of receptacles made of synthetic material or of glass shall not exceed 500 ml. Receptacles with a volume greater than 1 000 ml are therefore not permitted.