The following substances may not be carried in a type N vessel:

- substances with self-ignition temperatures <= 200 °C;
- substances with a flash point < 23°C and an explosion range > 15 percentage points;
- mixtures containing halogenated hydrocarbons;
- mixtures containing more than 10 % benzene;
- substances and mixtures carried in a stabilized state.