For an initial boiling point above 60 °C and under or equal to 85 °C as determined in accordance with ASTMD 86-01, the applicable conditions of transport are identical to those stipulated for an initial boiling point under or equal to 60 °C.