(a) While the vessel is underway, an inert-gas pad shall be maintained in the ullage space above the liquid level.

(b) Cargo piping and vent lines shall be independent of the corresponding piping used for other cargoes.

(c) Safety valves shall be made of stainless steel.