These substances may be carried in bulk if the results of the trough test according to subsection 38.2 of the Manual of Tests and Criteria show that the self-sustaining decomposition rate is not greater than 25 cm/h.