Battery mark:
Note: This mark is necessary for the transport of lithium cells or batteries or sodium ion cells or batteries according to special provision 188. In this case a label model No. 9A is not required.
The mark shall be in the form of a rectangle or a square with hatched edging. The dimensions shall be a minimum of 100 mm wide x 100 mm high and the minimum width of the hatching shall be 5 mm. The symbol (group of batteries, one damaged and emitting flame, above UN number(s) ) shall be black on white or suitable contrasting background. The hatching shall be red. If the size of the package so requires, the dimensions/line thickness may be reduced to not less than 100 mm wide x 70 mm high. Where dimensions are not specified, all features shall be in approximate proportion to those shown.

* Place for UN number(s)

Note: see Transitional measure 1.6.1.49

The mark shown in Figure 5.2.1.9.2 applicable until 31 December 2022, may continue to be applied until 31 December 2026.
