Multilateral Agreement ADN/M 030

under section 1.5.1 ADN Concerning the carriage of BUTADIENES AND HYDROCARBON MIXTURE, STABILIZED of Class 2


By derogation from 2.2.2.3, Table A and Table C of Chapter 3.2, it is allowed to transport mixtures of butadienes and hydrocarbon, with a concentration of butadienes of more than 20 % but not more than 40 %, stabilized, having a vapour pressure at 70 °C not exceeding 1.1 MPa (11 bar) and a density at 50 °C not lower than 0.525 kg/l under the designation of UN 1010 BUTADIENES AND HYDROCARBON MIXTURE, STABILIZED.

The consignor shall enter in the transport document

"Carriage agreed under the terms of section 1.5.1 of ADN (M030)".

This agreement shall be valid until 30 June 2025 for carriage on the territories of the ADN Contracting Parties signatory to this Agreement. If it is revoked before that date by one of the signatories, it shall remain valid until the above-mentioned date only for carriage on the territories of those ADN Contracting Parties signatory to this Agreement which have not revoked it.