See 2.2.2.3, classification code 2F, UN No. 1965, Note 2.

____
Note 2:
"UN No. 1075 PETROLEUM GASES, LIQUEFIED may be used as an alternative entry for UN No. 1965 HYDROCARBON GAS MIXTURE LIQUEFIED, N.O.S. for carriage prior to or following maritime or air carriage."