Carriage of this substance is permitted in tanks only.

Because the flash-point of 52°C c.c. is lower than the melting point (55°C), the melted substance must be transported under this UN No.
The solid substance has to be transported under UN No. 1325 (see BAM No. 12602).