Special packing provision PP84:
For UN No. 1057, rigid outer packagings meeting the packing group II performance level shall be used. The packagings shall be designed and constructed and arranged to prevent movement, inadvertent ignition of the devices or inadvertent release of flammable gas or liquid.

NOTE: For waste lighters collected separately see Chapter 3.3, special provision 654.


Special packing provision RR5 specific to ADR:
Notwithstanding special packing provision PP84, only the general provisions of 4.1.1.1, 4.1.1.2 and 4.1.1.5 to 4.1.1.7 need be complied with if the gross mass of the package is not more than 10 kg.

NOTE: For waste lighters collected separately see Chapter 3.3, special provision 654.