BAM has the result of a test report from a manufacturer; according to this, the substance, in addition to its corrosive properties, is also flammable in accordance with Class 4.1, packing group II. According to the Table of precedence of hazards, the substance was therefore assigned to Class 4.1, packing group II.