The general provisions of 4.1.1 and 4.1.3 shall be met.

Inner packagings made of plastics, paper or fibre shall be sift-proof.
Large outer packagings made of flexible plastics (51H) shall be used with flexible inner packagings only. 

Maximum capacity: 3 m³