Carriage of this substance is permitted in tanks only.
Tear gas substances shall be assigned to packing group II even if the data on their toxicity meet the criteria for packing group III. (see 2.2.61.1.7 and 2.2.61.1.8).