The following packagings are authorized, provided that the general provisions of 4.1.1 and 4.1.3 are met:

| Combination packagings                  | Inner packaging  | Outer packaging  |
|                                         | maximum capacity | maximum net mass |
+-----------------------------------------+------------------+------------------+
| Boxes (4A, 4B, 4N, 4C1, 4C2, 4D, 4H2)   |       5 l        |      125 kg      |
| or drums (1A1, 1A2, 1B1, 1B2, 1N1, 1N2, |                  |                  |
| 1H1, 1H2, 1D) or jerricans (3A1, 3A2,   |                  |                  |
| 3B1, 3B2, 3H1, 3H2) with glass,         |                  |                  |
| plastics or metal inner packagings      |                  |                  |
|                                         |                  |                  |
| Fibreboard box (4G) or fibre drum (1G), |       2 l        |      50 kg       |
| with plastics or metal inner packa-     |                  |                  |
| gings each in a plastics bag            |                  |                  |
+-----------------------------------------+------------------+------------------+

Additional requirements
1. Packagings shall have a maximum filling degree of 90 %.
2. Packagings shall be vented.