The general provisions of 4.1.1 and 4.1.3 shall be met.

The packagings listed are authorized, provided that explosion is not possible by reason of increased internal pressure. The maximum net mass shall not exceed 30 kg.