The design type shall be tested and marked appropriately.

Note:
In the opinion of BAM, light-gauge metal packagings of the design types 0A1 and 0A2 are not suitable for substances with a vapor pressure of more than 110 kPa. We do not recommend using these packagings for this substance, although packing instruction R001 is listed in Table A of ADR. The joint meeting has been informed.