The periodic inspections according to 6.8.2.4.2 shall be performed:
- fixed tanks (tank-vehicles), demountable tanks and battery-vehicles: no later than every three years;
- tank-containers, tank swap bodies and MEGCs: no later than every two and a half years.