Carriage of this substance is permitted in tanks only. This entry refers to the molten pure substance and not the commercial product that, according to some manufacturers, contains xylene and for which a flash-point of about 42°C c. c. is given.