According to 6.2.6.1.2 of the ADR, the capacity of receptacles made of metal shall not exceed 1 000 ml; that of receptacles made of synthetic material or of glass shall not exceed 500 ml. Receptacles with a volume greater than 1 000 ml are therefore not permitted.