See remarks 13) and 14) in sub-section 2.2.52.4:

13) "CORROSIVE" subsidiary hazard label required (Model No.8, see 5.2.2.2.2).

14) Peroxyacetic acid formulations which fulfil the criteria of the Manual of Tests and Criteria, paragraph 20.4.3 (d).