See remarks 13), 16) and 19) in sub-section 2.2.52.4:

13) "CORROSIVE" subsidiary hazard label required (Model No.8, see 5.2.2.2.2).

16) Peroxyacetic acid formulations which fulfil the criteria of the Manual of Tests and Criteria, paragraph 20.4.3 (f).

19) Mixtures with hydrogen peroxide, water and acid(s).