If the vehicle or container is made of wood or other combustible material, an impermeable
 surfacing resistant to combustion or a coating of sodium silicate or similar substance shall
 be provided. Sheeting shall also be impermeable and non-combustible.