Since this BAM number assumes that the substance liquefies during carriage, it may not be carried in IBCs under these circumstances (see also sub-section 4.1.3.4 of ADR).

However, provided the substance does not melt during carriage, carriage in IBCs is permitted (see the relevant BAM number with the suffix "solid").