See remark 1) in sub-section 2.2.52.4:
"Diluent type B may always be replaced by diluent type A. The boiling point of diluent type B shall be at least 60 °C higher than the SADT of the organic peroxide."

Note: This remark applies only to the carriage of organic peroxides in packagings.