Pressure receptacles shall satisfy the following conditions:

(a) The pressure test shall include an inspection of the inside of the pressure receptacles and check of accessories;

(b) In addition resistance to corrosion shall be checked every two years by means of suitable instruments (e.g. ultrasound) and the condition of the accessories verified;

(c) Wall thickness shall not be less than 3 mm.