For UN Nos. 0248 and 0249, packagings shall be protected against the ingress of water. When water-activated contrivances are transported unpackaged, they shall be provided with at least two independent protective features which prevent the ingress of water.

NOTE: The packagings authorized may exceed a net mass of 400 kg (see 4.1.3.3).