See remarks 3) and 13) in sub-section 2.2.52.4:

3) "EXPLOSIVE" subsidiary hazard label required (Model No.1, see 5.2.2.2.2).

13) "CORROSIVE" subsidiary hazard label required (Model No.8, see 5.2.2.2.2).