The maximum degree of filling (in %) for solids carried above their melting point and for elevated temperature liquids shall be determined in accordance with 4.2.1.9.5.

Degree of filling = 95 x ( dr / df )

where
dr = density of the liquid during carriage;
df = density of the liquid during filling [°C].