There are indications that it may be toxic by inhalation. However, the data situation is not sufficient for a reliable classification.
If classification in Class 6.1 is not required, the substance shall be assigned to UN No. 3257 if it is carried or handed over for carriage at a temperature above 100°C and to UN No. 3256 if the temperature is 125°C or above.