Carriage of this substance is permitted in tanks only.

This classification applies only to carriage below the flash-point. When transported at a temperature at or above the flash-point, the Class 3 hazard must also be considered.