Because the substance is classified according to Regulation (EC) No 1272/2008 (CLP Regulation) with 1. ATP to 6. ATP in the subcategory "corrosive Cat. 1B",  BAM assigned it to Class 8, packing group II. If different data are available to the user, classification in packing group III may be possible.