Code LGAV:

L = Type of tank:

Tank for substances in the liquid state (liquids or solids handed over for carriage in the molten state).
-------------------------

G = Calculation pressure:

Minimum calculation pressure according to the general requirements of 6.8.2.1.14.
-------------------------

A = Openings (see 6.8.2.2.2):

Tank with bottom-filling or bottom-discharge openings with 2 closures.
-------------------------

V = Safety valves/devices:

Tank with a breather device, according to 6.8.2.2.6, but no device protecting against the propagation of a flame; or non-explosion pressure shock resistant tank.