The following packagings are authorized provided the general provisions of 4.1.1 and 4.1.3 are met:

| Inner packagings  |   Outer packagings    |   Code   | Maximum * |
+-------------------+-----------------------+----------+-----------+
| Glass       10 kg | Drums                 |          |           |
| Plastics 1) 50 kg |    steel              | 1A1, 1A2 |  400 kg   |
| Metal       50 kg |    aluminium          | 1B1, 1B2 |  400 kg   |
| Paper 1),2) 50 kg |    other metal        | 1N1, 1N2 |  400 kg   |
| Fibre 1),2) 50 kg |    plastics           | 1H1, 1H2 |  400 kg   |
|                   |    plywood            | 1D       |  400 kg   |
|                   |    fibre              | 1G       |  400 kg   |
|                   +-----------------------+----------+-----------+
|                   | Boxes                 |          |           |
|                   |    steel              | 4A       |  400 kg   |
|                   |    aluminium          | 4B       |  400 kg   |
|                   |    other metal        | 4N       |  400 kg   |
|                   |    natural wood       | 4C1      |  400 kg   |
|                   |    natural wood with  | 4C2      |  400 kg   |
|                   |      sift-proof walls |          |           |
|                   |    plywood            | 4D       |  400 kg   |
|                   |    reconstituted wood | 4F       |  400 kg   |
|                   |    fibreboard         | 4G       |  400 kg   |
|                   |    expanded plastics  | 4H1      |   60 kg   |
|                   |    solid plastics     | 4H2      |  400 kg   |
|                   +-----------------------+----------+-----------+
|                   | Jerricans             |          |           |
|                   |    steel              | 3A1, 3A2 |  120 kg   |
|                   |    aluminium          | 3B1, 3B2 |  120 kg   |
|                   |    plastics           | 3H1, 3H2 |  120 kg   |
+-------------------+-----------------------+----------+-----------+

* Maximum net mass (see 4.1.3.3)

1) These inner packagings shall be sift-proof.
2) These inner packagings shall not be used when the substances being carried may become liquid during carriage (see 4.1.3.4).