Carriage of this substance is permitted in tanks only.

According to the findings of BAM, 2,6- and 3,5-dinitrotoluene are not environmentally hazardous in the sense of the dangerous goods regulations.