The following packagings are authorized, provided that the general provisions of 4.1.1 and 4.1.3 are met:

| Inner packagings |    Outer packagings   |   Code   | Maximum * |
+------------------+-----------------------+----------+-----------+
| Glass       5 kg | Drums                 |          |           |
| Metal       5 kg |    steel              | 1A1, 1A2 |  125 kg   |
| Plastics    5 kg |    aluminium          | 1B1, 1B2 |  125 kg   |
|                  |    other metal        | 1N1, 1N2 |  125 kg   |
|                  |    plastics           | 1H1, 1H2 |  125 kg   |
|                  |    plywood            | 1D       |  125 kg   |
|                  |    fibre              | 1G       |  125 kg   |
|                  +-----------------------+----------+-----------+
|                  | Boxes                 |          |           |
|                  |    steel              | 4A       |  125 kg   |
|                  |    aluminium          | 4B       |  125 kg   |
|                  |    other metal        | 4N       |  125 kg   |
|                  |    natural wood       | 4C1      |  125 kg   |
|                  |    natural wood with  | 4C2      |  125 kg   |
|                  |      sift-proof walls |          |           |
|                  |    plywood            | 4D       |  125 kg   |
|                  |    reconstituted wood | 4F       |  125 kg   |
|                  |    fibreboard         | 4G       |   40 kg   |
|                  |    expanded plastics  | 4H1      |   60 kg   |
|                  |    solid plastics     | 4H2      |  125 kg   |
+------------------+-----------------------+----------+-----------+

* Maximum net mass