Carriage of this substance is permitted in tanks only.

This substance is classified as "environmentally hazardous" and "skin corrosive Cat. 1B" in accordance with Regulation (EC) No 1272/2008 (CLP Regulation). This corresponds to the criteria of packing group II. BAM has no further data on corrosivity. The consignor must decide whether the packing group is sufficient for the substance to be shipped.