Carriage of this substance is permitted under packing group II if the boiling point is greater than 35°C (see BAM No. 12580). With a boiling point not exceeding 35°C, it has to be assigned to packing group I.