The following packagings are authorized provided the general provisions of 4.1.1 and 4.1.3 are met (only "soft" packagings of packing instruction P001):

| Inner packagings  |   Outer packagings     |   Code   | Maximum * |
+-------------------+------------------------+----------+-----------+
| Plastics 1) 50 kg | Drums                  |          |           |
| Paper 1)    50 kg |    plastics            | 1H1, 1H2 |  400 kg   |
| Fibre 1)    50 kg |    plywood             | 1D       |  400 kg   |
|                   |    fibre               | 1G       |  400 kg   |
|                   +------------------------+----------+-----------+
|                   | Boxes                  |          |           |
|                   |    natural wood        | 4C1      |  400 kg   |
|                   |    natural wood with   | 4C2      |  400 kg   |
|                   |      sift proof walls  |          |           |
|                   |    plywood             | 4D       |  400 kg   |
|                   |    reconstituted wood  | 4F       |  400 kg   |
|                   |    fibreboard          | 4G       |  400 kg   |
|                   |    expanded plastics   | 4H1      |   60 kg   |
|                   |    solid plastics      | 4H2      |  400 kg   |
|                   +------------------------+----------+-----------+
|                   | Jerricans              |          |           |
|                   |    plastics            | 3H1, 3H2 |  120 kg   |
|-------------------+------------------------+----------+-----------+

* Maximum capacity/Net mass (see 4.1.3.3)

1) These inner packagings shall be sift-proof.