According to 2.2.2.2.2 sixth indent, Aerosols where gases which are toxic according to 2.2.2.1.5 or pyrophoric according to packing instruction P200 in 4.1.4.1 are used as propellants, shall not be accepted for carriage.