The concentration specification is based on information in the ICAO TI; here, the substance may be transported only up to a concentration of 49%. However, in Regulation (EC) No 1272/2008 (CLP Regulation), assignment to packing group II applies only up to a concentration of 40%. BAM has no further information on this matter.