Aluminium alloy pressure receptacles shall be:

(a) Equipped only with brass or stainless steel valves; and

(b) Cleaned for hydrocarbons contamination and not contaminated with oil. UN pressure receptacles shall be cleaned in accordance with ISO 11621:1997.