Tixed tanks (tank-vehicles), demountable tanks and battery-vehicles:
The hydraulic pressure tests shall be performed no later than every 3 years.

Tank-containers, tank swap bodies and MEGCs:
The hydraulic pressure tests shall take place at least every 2,5 years.