The general provisions of 4.1.1, 4.1.2 and 4.1.3 shall be met.

Special packing provision B19:
For UN Nos. 3532 and 3534, IBCs shall be designed and constructed to permit the release of gas or vapour to prevent a build-up of pressure that could rupture the IBCs in the event of loss of stabilization.