The following packagings are authorized, provided that the general provisions of 4.1.1 and 4.1.3 are met:

| Combination packagings                         | Maximum * |
+------------------------------------------------+-----------+
| (1) Glass receptacles with a maximum capacity  |   75 kg   | 
| of 5 litres in 1A1, 1A2, 1B1, 1B2, 1N1, 1N2,   |           |
| 1H1, 1H2, 1D, 1G, 4A, 4B, 4N, 4C1, 4C2, 4D,    |           |
| 4F, 4G, 4H2 outer packagings                   |           |
|                                                |           |
| (2) Plastics receptacles with a maximum        |   75 kg   |
| capacity of 30 litres in 1A1, 1A2, 1B1, 1B2,   |           |
| 1N1, 1N2, 1H1, 1H2, 1D, 1G, 4A, 4B, 4N, 4C1,   |           |
| 4C2, 4D, 4F, 4G, 4H2 outer packagings          |           |
|                                                |           |
| (3) Metal receptacles with a maximum capacity  |   125 kg  |
| of 40 litres in 1G, 4F or 4G outer packagings  |           |
|                                                |           |
| (4) Metal receptacles with a maximum capacity  |   225 kg  |
| of 40 litres in 1A1, 1A2, 1B1, 1B2, 1N1, 1N2,  |           |
| 1H1, 1H2, 1D, 4A, 4B, 4N, 4C1, 4C2, 4D, 4H2    |           |
| outer packagings                               |           |
+------------------------------------------------+-----------+

*) Maximum net mass