This substance may only be transported under packing group II if the boiling point is greater than 35 °C!
If the substance has a maximum boiling point of 35 °C, it is to be assigned to packing group I (see BAM No. 12656).