Only cryogenic receptacles are authorized (see topic "Single packagings").

Open cryogenic receptacles of glass double wall construction shall have an outer packaging with suitable cushioning or absorbent materials which withstand the pressures and impacts liable to occur under normal conditions of carriage.