This substance is listed in tank instruction T23 in 4.2.5.2.6 of the ADR. Since 1 January 2019, the substances listed in tank instruction T23 may also be carried packed in accordance with packing method OP8 of packing instruction P520 of 4.1.4.1, with the same control and emergency temperatures, if applicable.

Since this substance is also listed in the table in sub-section 2.2.52.4, it may be transported in packagings under UN No. 3109 mentioned there, even without temperature control. A second BAM No. 10146 exists for this.