The following packagings are authorized, provided the general provisions of 4.1.1 and 4.1.3 are met:

For liquids containing or contaminated with PCBs, polyhalogenated biphenyls, polyhalogenated terphenyls or halogenated monomethyldiphenylmethanes: Packagings in accordance with packing instruction P001 (see below).

Notwithstanding the above, liquids not packaged in accordance with packing instruction P001 may be carried in cargo transport units fitted with a leakproof metal tray to a height of at least 800 mm, containing sufficient inert absorbent material to absorb at least 1.1 times the volume of any free liquid.

NOTE: The packagings authorized may exceed a net mass of 400 kg (see 4.1.3.3).


Combination packagings according to packing instruction P001:

| Inner packagings |   Outer packagings    |   Code   | Maximum * |
+------------------+-----------------------+----------+-----------+
| Glass       10 l | Drums                 |          |           |
| Plastics    30 l |    steel              | 1A1, 1A2 |  400 kg   |
| Metal       40 l |    aluminium          | 1B1, 1B2 |  400 kg   |
|                  |    other metal        | 1N1, 1N2 |  400 kg   |
|                  |    plastics           | 1H1, 1H2 |  400 kg   |
|                  |    plywood            | 1D       |  400 kg   |
|                  |    fibre              | 1G       |  400 kg   |
|                  +-----------------------+----------+-----------+
|                  | Boxes                 |          |           |
|                  |    steel              | 4A       |  400 kg   |
|                  |    aluminium          | 4B       |  400 kg   |
|                  |    natural wood       | 4C1, 4C2 |  400 kg   |
|                  |    plywood            | 4D       |  400 kg   |
|                  |    reconstituted wood | 4F       |  400 kg   |
|                  |    fibreboard         | 4G       |  400 kg   |
|                  |    expanded plastics  | 4H1      |   60 kg   |
|                  |    solid plastics     | 4H2      |  400 kg   |
|                  +-----------------------+----------+-----------+
|                  | Jerricans             |          |           |
|                  |    steel              | 3A1, 3A2 |  120 kg   |
|                  |    aluminium          | 3B1, 3B2 |  120 kg   |
|                  |    plastics           | 3H1, 3H2 |  120 kg   |
+------------------+-----------------------+----------+-----------+

* Maximum net mass