The general provisions of 4.1.1 except 4.1.1.15 and 4.1.3 shall be met.

Packagings shall conform to the packing group II performance level for solids.

Additional requirement:
Packagings intended to contain sharp objects such as broken glass and needles shall be resistant to puncture and retain liquids under the performance test conditions in Chapter 6.1.